**SILVER LINE PRODUCT SPECIFICATIONS**

**A picture containing handwear, clothing

Description generated with very high confidence**

**Product Salience**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **Name of Product** | **:** 14 Mil Powder Free Latex house hold Gloves. | | | | |
| **Name of Manufacturer** : :Innovative Gloves Co. Ltd. Hatyai, Thailand | | | | |
| **Base Material** | : Natural latex |  |
| **Characteristics** | : Non Sterile, Ambidextrous Beaded Cuff | | | |
| **Available Sizes** | : X-small, Small, Medium, Large, X-Large , XX- Large | | |
| **Surface** | : Diamond Textured. | |
| **Surface Treatment** | : Mild washing with chlorine solution and extensive washing | |
| **Colour** | : white and Blue |  |

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Physical Specifications:** | | | | | |  |  |  |  |  |  |  |  |  |  |  |  |
|  |  |  | Length | |  | SINGLE WALL (mm) | | | | | | | | |  | Width |  |
|  | Size | |  | Cuff |  | Palm | |  |  |  |  | Tip | |  |
|  | (mm) | |  |  |  |  |  |  | (mm) |  |
|  |  |  |  | Smooth |  | Textured | |  |  | Smooth | | | Textured |  |
|  |  |  |  |  |  |  |  |  |  |  |
|  |  |  |  |  |  | Surface |  | Surface | |  |  | Surface | | | Surface |  |  |
|  | Medium (8) | | 300±10 | |  | 0.21±0.01 |  | 0.65±0.05 | |  | 0.37±0.01 | | | | 0.60±0.05 | 100±5 |  |
|  |  | |  | |  |  |  |  | |  |  | | | |  |  |  |
|  | Large (9) | | 300±10 | |  | 0.21±0.01 |  | 0.65±0.05 | |  | 0.37±0.01 | | | | 0.60±0.05 | 115±5 |  |
|  | X Large (10) | | 300±10 | |  | 0.21±0.01 |  | 0.65±0.05 | |  | 0.37±0.01 | | | | 0.60±0.05 | 120±3 |  |
|  | XX Large (11) | | 300±10 | |  | 0.21±0.01 |  | 0.65±0.05 | |  | 0.37±0.01 | | | | 0.60±0.05 | 125±3 |  |

|  |  |  |
| --- | --- | --- |
| **Tensile(MPA)** | **Elongation(%)** | **Force At Break(N)** |
|  |  |  |

**Tensile (ASTM D 6319 & EN 455-2)**

**Quality Assurance**

|  |  |
| --- | --- |
| **Visual Inspection G-I AQL** | **Physical dimension S-II AQL** |
| **Leak Test G-I AQL** | **Physical Properties S-II AQL** |

**International Compliances:**

* CE:
* Sizing, Dexterity & Mechanical Attribute:
* Innocuousness & PH:
* Microbial Penetration & chemical Permeation:
* Food Safe Application:

|  |  |  |  |
| --- | --- | --- | --- |
| **Total Residue Content** | | - < 2.0 Milligrams per glove |  |
| **Packaging (Normal)** | | - 50 pieces in one Poly Bag or Dispenser Box | |
|  |  | 10 Poly Bag or Dispenser Box in one Carton | |

**Labeling on Dispenser (Normal)** - Product Name, Size, Lot no. Quantity, Manufacturer’s address.

**Labeling on Carton (Normal)** - Product Name, Size, Lot no. Quantity, Country of Origin

**Container Loadability** (No MOQ in manufacturer owned brand in standard Packaging)

20FCL=800 Cases,40 FCL=1600 Cases,40FCL-Q=1900 Cases.